**Chapter I LDMStudio Installation**

REMARKS: Please close your antivirus programs before the installation, in case of wrong warnings from your antivirus programs.

1. **Contents in the Disc:**



**LDMStudio:** Packed Program, please just copy it to your computer. Installation is not needed here;

**LDMStudio\_setup:** Installation Program;


**readme.docx:** Installation Instruction in 2007 version Words;

**readme.pdf:** Installation Instruction in .pdf.


1. **Software Installation**
   1. Open the folder LDMStudio\_setup, double click setup.exe to start the installing

****


* 1. Click “Next>” when you get the below interface;

****


* 1. Enter the user name and company name, and then click “Next>”




* 1. Click “Complete”, the program will choose a default path for the installation; we choose “Custom” and click “Next>” for example.




* 1. Click Browse to revise the installing path, and then click “Nest>”.




* 1. Click “Next>” to continue.



* 1. Click “Install” to start the installation.




* 1. Click “Finish”. The Installation is completed.




1. **Program Uninstallation**
   1. Installation and Uninstallation is the same file. Open folder LDMStudio\_setup, double click setup.exe to start uninstalling.

****


* 1. Select “Remove” and then click “Next>”.



* 1. Click “Y” when you get the below interface.

****

* 1. Click “Finish” to end the uninstalling.




**Chapter II Program Instruction**

1. **Connect the meter with PC.**
   1. Double click the icon LDMStudio to run the program



* 1. Interface of the Program



* 1. Connect the meter and PC with USD connector.



* 1. “Connected OK” will be shown at the left bottom of the interface when the connection is successful. The buttons in the interface can be operated.



1. **Opertation**
   1. Obtain the measuring data.

Click “Read” once, laser release, click “Read” again to get the result.

C:\Documents and Settings\Administrator\桌面\未标题-1.bmp

* 1. Clear up the measuring data.


Click “Clear” to clear up the data on the screen.

C:\Documents and Settings\Administrator\桌面\未标题-2.bmp

* 1. Obtain the measuring record.

Click “Export Records” to deliver the measuring records to the program.






* 1. Click “Export to Excel”, revise the file name and path in the popup and then click “save” to upload the measuring records to PC in .xlsx file.




* 1. Print the records.
     1. Press “Print” after uploading.



* + 1. Click “OK” to preview.



* + 1. Preview Interface



* + 1. Click “Print”.



* + 1. Click “OK” for printing.

